!

! Last configuration change at 21:41:23 CET Sun Mar 27 2016

!

version 15.2

service timestamps debug datetime msec

service timestamps log datetime msec

no service password-encryption

service compress-config

!

hostname SW3

!

boot-start-marker

boot-end-marker

!

!

logging discriminator EXCESS severity drops 6 msg-body drops EXCESSCOLL

logging buffered 50000

logging console discriminator EXCESS

!

no aaa new-model

clock timezone CET 1 0

!

!

!

!

!

vtp mode transparent

no ip icmp rate-limit unreachable

!

!

!

ip cef

no ip igmp snooping

no ipv6 cef

!

!

!

spanning-tree mode rapid-pvst

spanning-tree extend system-id

!

vlan internal allocation policy ascending

!

vlan 2-10,12,23,34,45,67,78,89,109,144,235,456

!

ip tcp synwait-time 5

!

!

!

!

!

!

!

!

!

!

!

!

!

interface Ethernet0/0

switchport trunk encapsulation dot1q

switchport mode trunk

spanning-tree portfast edge trunk

!

interface Ethernet0/1

switchport trunk encapsulation dot1q

switchport mode trunk

spanning-tree portfast edge trunk

!

interface Ethernet0/2

switchport trunk encapsulation dot1q

switchport mode trunk

spanning-tree portfast edge trunk

!

interface Ethernet0/3

switchport trunk encapsulation dot1q

switchport mode trunk

spanning-tree portfast edge trunk

!

interface Ethernet1/0

switchport trunk encapsulation dot1q

switchport mode trunk

spanning-tree portfast edge trunk

!

interface Ethernet1/1

switchport trunk encapsulation dot1q

switchport mode trunk

spanning-tree portfast edge trunk

!

interface Ethernet1/2

switchport trunk encapsulation dot1q

switchport mode trunk

spanning-tree portfast edge trunk

!

interface Ethernet1/3

switchport trunk encapsulation dot1q

switchport mode trunk

spanning-tree portfast edge trunk

!

interface Ethernet2/0

switchport trunk encapsulation dot1q

switchport mode trunk

!

interface Ethernet2/1

switchport trunk encapsulation dot1q

switchport mode trunk

!

interface Ethernet2/2

switchport trunk encapsulation dot1q

switchport mode trunk

spanning-tree link-type point-to-point

!

interface Ethernet2/3

switchport trunk encapsulation dot1q

switchport mode trunk

spanning-tree link-type point-to-point

!

interface Ethernet3/0

switchport trunk encapsulation dot1q

switchport mode trunk

spanning-tree link-type point-to-point

!

interface Ethernet3/1

switchport trunk encapsulation dot1q

switchport mode trunk

spanning-tree link-type point-to-point

!

interface Ethernet3/2

switchport trunk encapsulation dot1q

switchport mode trunk

spanning-tree link-type point-to-point

!

interface Ethernet3/3

switchport trunk encapsulation dot1q

switchport mode trunk

spanning-tree link-type point-to-point

!

interface Vlan1

ip address 10.0.0.103 255.255.255.0

no shutdown

!

ip forward-protocol nd

!

no ip http server

no ip http secure-server

!

!

!

!

!

!

control-plane

!

banner motd ^C

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\*\*\*\*\*\*\*\*\*\* LAB 44 TASK 1 \*\*\*\*\*\*\*\*\*\*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

^C

!

line con 0

exec-timeout 0 0

privilege level 15

logging synchronous

transport preferred none

line aux 0

line vty 0 4

privilege level 15

no login

transport preferred none

transport input telnet

!

!

end